metadata contain GPS exact location of camera 
+ exact altitude above sea level - see atributes

to adjust properly camera when implementing visualisation or model set following:

nescessary
Field Of View	73.7 deg
Focal Length	4.4 mm (35 mm equivalent: 24.0 mm)

optional
Hyperfocal Distance	1.25 m